F0 00 00 50 29 00 F7
{ Clear All Settings - allow all MIDI events not specified below to pass through unchanged }

F0 00 00 50 29 02 00 00 02 30 3F 01 03 00 7F F7
90 00 00
B0 63 20
{ Setting #1: Map Note-on #48 - 63 events on MIDI channel 1 to Control Change #99 of value 32 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 01 00 02 30 3F 01 03 00 7F F7
90 00 00
B0 62 01
{ Setting #2: Map Note-on #48 - 63 events on MIDI channel 1 to Control Change #98 of value 1 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 02 01 03 00 7F F7
90 30 00
B0 06 05
{ Setting #3: Map all Note-on #48 events on MIDI channel 1 to Control Change #6 of value 5 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 03 01 03 00 7F F7
90 31 00
B0 06 0A
{ Setting #4: Map all Note-on #49 events on MIDI channel 1 to Control Change #6 of value 10 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 04 01 03 00 7F F7
90 32 00
B0 06 13
{ Setting #5: Map all Note-on #50 events on MIDI channel 1 to Control Change #6 of value 19 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 05 01 03 00 7F F7
90 33 00
B0 06 1B
{ Setting #6: Map all Note-on #51 events on MIDI channel 1 to Control Change #6 of value 27 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 06 01 03 00 7F F7
90 34 00
B0 06 24
{ Setting #7: Map all Note-on #52 events on MIDI channel 1 to Control Change #6 of value 36 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 07 01 03 00 7F F7
90 35 00
B0 06 2C
{ Setting #8: Map all Note-on #53 events on MIDI channel 1 to Control Change #6 of value 44 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 08 01 03 00 7F F7
90 36 00
B0 06 33
{ Setting #9: Map all Note-on #54 events on MIDI channel 1 to Control Change #6 of value 51 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 09 01 03 00 7F F7
90 37 00
B0 06 3A
{ Setting #10: Map all Note-on #55 events on MIDI channel 1 to Control Change #6 of value 58 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 0A 01 03 00 7F F7
90 38 00
B0 06 43
{ Setting #11: Map all Note-on #56 events on MIDI channel 1 to Control Change #6 of value 67 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 0B 01 03 00 7F F7
90 39 00
B0 06 4B
{ Setting #12: Map all Note-on #57 events on MIDI channel 1 to Control Change #6 of value 75 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 0C 01 03 00 7F F7
90 3A 00
B0 06 54
{ Setting #13: Map all Note-on #58 events on MIDI channel 1 to Control Change #6 of value 84 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 0D 01 03 00 7F F7
90 3B 00
B0 06 5B
{ Setting #14: Map all Note-on #59 events on MIDI channel 1 to Control Change #6 of value 91 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 0E 01 03 00 7F F7
90 3C 00
B0 06 63
{ Setting #15: Map all Note-on #60 events on MIDI channel 1 to Control Change #6 of value 99 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 0F 01 03 00 7F F7
90 3D 00
B0 06 6C
{ Setting #16: Map all Note-on #61 events on MIDI channel 1 to Control Change #6 of value 108 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 10 01 03 00 7F F7
90 3E 00
B0 06 74
{ Setting #17: Map all Note-on #62 events on MIDI channel 1 to Control Change #6 of value 116 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 11 01 03 00 7F F7
90 3F 00
B0 06 7D
{ Setting #18: Map all Note-on #63 events on MIDI channel 1 to Control Change #6 of value 125 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 12 01 03 00 7F F7
90 40 00
B0 63 20
{ Setting #19: Map all Note-on #64 events on MIDI channel 1 to Control Change #99 of value 32 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 13 01 03 00 7F F7
90 40 00
B0 62 02
{ Setting #20: Map all Note-on #64 events on MIDI channel 1 to Control Change #98 of value 2 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 14 01 03 00 7F F7
90 40 00
B0 06 7F
{ Setting #21: Map all Note-on #64 events on MIDI channel 1 to Control Change #6 of value 127 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 15 01 03 00 7F F7
90 41 00
B0 63 20
{ Setting #22: Map all Note-on #65 events on MIDI channel 1 to Control Change #99 of value 32 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 02 16 01 03 00 7F F7
90 41 00
B0 62 11
{ Setting #23: Map all Note-on #65 events on MIDI channel 1 to Control Change #98 of value 17 on MIDI channel 1. Continue to process settings }

F0 00 00 50 29 0A 17 01 03 00 7F F7
90 41 00
B0 06 7F
{ Setting #24: Map all Note-on #65 events on MIDI channel 1 to Control Change #6 of value 127 on MIDI channel 1. If this setting is executed, stop processing settings }